|  |  |
| --- | --- |
| **Phase Locked Oscillator****Internal Reference** | **MODEL: PmT-3220-Frequency (GHz)** |
| **Features:*** Small Size
* Excellent Phase Noise
* Low Cost
* Crystal Frequency Stability
* Phase Locked Resonator Oscillator
* SMT Fabrication
* Low Phase Noise
* Packaged Active Devices
 |
| **Electrical Specifications** |
| **Model: PmT-3220-Frequency (GHz)** |
| **Parameters** | **Specifications** |
| Frequency Range | 0.3 to 24 GHz |
| Power Output | +14 dBm |
| Load VSWR | 2.0:1 |
| Spurious | -70dBc max |
| Harmonics | -25 dBc |
| Alarm | High Z |
| Phase Noise10 KHz Offset100 KHz Offset1 MHz Offset | Reference Dependent-120 dBc/Hz140 dBc/Hz |
| Reference Input Frequency | N/A |
| Reference Input Power | N/A |
| Frequency Stability | Same as Ext Ref |
|  Voltage | 12/15 V |
|  Current | 300 mA |
| Package Outline  | Figure 102 |
| Connector | SMA-F |
| Operating Temperature | -25 to 70 °C |
| Storage Temperature | -55 to 125°C  |
| Size (inches) | 2.25 x 2.25 x 0.62 inches |
| Finish | Nickel Plated |